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1. OBJECTIVE:


1.1 The objective of this service program is to explain the implementations to be performed by the Directorate of Directives in scope of Regulation on Children Toys (2009/48/EC, BD-131704-01), referred to as Regulation hereinafter. 

1.2 This service program is in conformity with Type 1a certification program according to TS EN ISO/IEC 17067.

2.SCOPE
This service program includes conformity assessment procedures, authorized by the Directorate of Directives, for defined products in the part “Scope”, set out in Clause 2 of Regulation on Children Toys. 

2.1 Notified Body Criteria

BD09100502 - GSO Guide on Notified Bodies
2.2. Source Legislation

2009/48/EC Council Directive Safety of Toys (Official Journal No. L170/1 of 30 June 2009), 

BD-131704-01 GSO Technical Regulation on Toys:

 HYPERLINK "http://www.gso.org.sa/gso-website/gso-website/activities/conformity/technical-regulations-and-guides/bd-131704-01-en-08-09-13.pdf" 
 Second Edition 
2.3 Product groups

All children toys in scope with the Regulation.

Products shall be subjected to conformity assessment procedure by carrying out required stages according to the declared modules and procedures in flow chart in part 7 and in part 4.

3. RESPONSIBLE DEPARTMENTS:

Head of the Center
Head of Group
Director of Directives
Directive Responsible
Directive Experts

GCC Legal Representative
 4. IMPLEMENTATION

4.1. Stages of Conformity Assessment Procedure

4.1.1. Acceptance of Applications

According to Conformity Assessment Application Procedure, applications shall be made to TSE with the Toys Conformity Assessment Application Form and the Technical File, and with other documents and files required by the certification procedure, which are chosen by the manufacturer.
Application File shall be assessed according to Conformity Assessment Application Procedure. As a result of assessment, certification procedures shall be initiated for files, which are deemed appropriate for conformity assessment services.
4.1.2 Modules and Implementations

4.1.2.1 Introduction

Conformity assessment processes are given in flow charts in Clause 6 of this service program. Conformity assessment models in these charts are described as following: 
4.1.2.2. Conformity Assessment - Manufacturer 

According to Annex IV Toys TR;

Manufacturer Internal Production Control: 

It is applied for the toys for which the Manufacturer has chosen to apply solutions under the scope of relevant Gulf standards; GSO NB may be involved voluntarily to control Manufacturer’s internal production.

Type Examination

Type examination; the examination and certification of the conformity of a toy to be produced, design documents and a product to be referred as type hereinafter to the provisions of the regulation shall be made in accordance with Module B Conformity Assessment Procedure. 

The below documents prepared by the manufacturer are verified by TSE:

1. Manufacturer conducts risk assessment, or have it conducted, and identifies significant aspects of risks in toys;

2. Manufacturer prepares the technical documentation according to the technical regulation (BD-

131704-01) Annex (IV) including:

a. List of risks and hazards in the toy and the listing of applied Gulf standards the toy complies with

according to the risk analysis according to point (a),

b. Bill of Materials,

c. The necessary test reports for significant risks identified,

d. A description of the procedures followed by the manufacturer to ensure the efficiency of factory

production control to achieve the conformity of the manufactured toys with the design specified in the

technical documents;

e. A declaration regarding the conformity of the products.

Whenever required, TSE can arrange necessary grouping, testing (fully or partially or on representative items) or technical assessment for the manufacturers. 

f. Labeling in Arabic language

(In the absence of an Arabic-speaking person, the evaluator will verify it using AI tools (ChatGPT Pro). The previously approved labels (i.e. those approved by the person) and the DB-TSD-FR-009 Toy Safety Warnings languages comparison table were first provided to the AI to ensure the correct terminology is used when comparing the Arabic labelling with the English/Turkish labelling.)

Criteria of grouping

a. Same HS code,

b. Similar age range,

c. Same manufacturer (same supplier). Same manufacturer may sell same toy using different brand names. This also can be grouped,

d. Same country,

e. Similar function and material.

f. There is no limit for the number of SKU if they meet above criteria.

Applicable Standards

Current Gulf standards and SASO standards are available online on https://www.gso.org.sa/store/gso/standards?lang=en and https://wasif.saso.gov.sa/Pages/User/Default.aspx respectively.
For the publication date of international standards can be seen from the standardization bodies websites: www.iso.org, standards.cen.eu, etc.

1. The following international standards (series) are adopted by the GSO and shall be applied in the preferential order as shown below:

a. GSO EN 71 set, EN 71 set is accepted;

b. IEC 62115, EN 62115 will require an additional gap analysis against GTTR essential requirement;

c. ISO 8124-series, additional tests may be required;

d. ASTM F963, additional tests may be required;

2. Adopt the updated version of standards. When new standard published, GSO can accept a grace period of 2 years after the publish date.

3. See the harmonised standards for presumption of conformity: https://www.gso.org.sa/nb/hs/BD-131704-01
Maximum Acceptance Period for Test Results:

a) Test reports generally shall be considered valid evidence if they clearly relate to the applied products and those reports bear the endorsement logo of a reputable accreditation body being a member of the ILAC multilateral agreement and only if obtained within a period no longer than 3 years prior to the date of the manufacturer’s application for G-Mark certification to the Notified Body.

b) Effective immediately, test results utilized for Gulf Type Examination certification will be considered valid if obtained within a period not exceeding three years from the date of actual test performance. This period is determined from the date when testing activities were completed and issued the test report, as explicitly stated in the laboratory testing report.

c) The issue date of the laboratory testing report may be later than the date of completion of testing, which is the date to be considered for calculating the 3 years period.

d) Any re-issuance of test report shall fulfil ISO/IEC 17025 relevant requirements. For example, test reports shall be re-issued only for the correction of errors and the inclusion of omitted data available at the time of tests.

Note: The practice which consists, in some accredited laboratories, of re-issuing a test report under accreditation coverage after the end of three years from the end date of performing the test (without re-testing) is not permitted, even with a clear reference to the initial report that it replaces.

e) The validity periods of the applied Harmonized Standards are not affected by this rule and must always be observed.

f) In cases where the test report does not directly correspond to the product model applied for certification, a Product Identity Declaration (PID) or Declaration of Identity (DOI) shall be provided showing the correlation, similarities and differences between the products applied for certification and the tested products and include the references to all test reports that show the relevant test results.

The PID/DOI shall be signed by an authorized person on behalf of the manufacturer or his authorized representative (e.g. technical responsible or top management representative) and issued on an official letter showing the name and address of the issuing company. PID/DOI shall be included in the certification documentation as submitted to the GCTS platform ( For detailed information please refer to GSO Announcement on 03.04.2024)

g) Whenever the NB has concerns as to the validity or authenticity of a test report presented by the manufacturer or importer, necessary testing may be arranged by the NB in agreement with the manufacturer
As a result of the examination, GCC Technical Regulation on Children Toys (BD131704-01) Essential Requirements Conformity Assessment Report shall be prepared and, shall be notified to the applicant with the test report if it’s not provided by the client. The report is numbered according to Clause 4.3 of the “BM-TL-005 Certification Services Traceability Instruction '.

In the event that the result of conformity assessment of the type is positive, Type Examination Certificate shall be issued with validity of 5 years. The manufacturer shall attach GC mark to each children toy conforming with Gulf technical regulations and issue Conformity Declaration in accordance with Clause 15 (1) of the Regulation.

If there is an application of the same product with different brand/ trademark, it’s needed the applicant to provide “Declaration of identification” to ensure that raw material and components used in each model of products subject to new application have the same properties as regards quality and innocuousness and are the same with the certified products. Upon on declaration of manufacturer, DB-FR-007 Result Evaluation Form is prepared by the directive expert by taking account of GCC Technical Regulation on Children Toys (BD131704-01) Essential Requirements Conformity Assessment Report which was prepared previously for the certified products and it is submitted for final decision of Conformity Assessment Committee. Following the decision, certification process is carried out in line with Clause 4.3. 

4.1.2.3. Conformity Assessment- Confirmation of Conformity of the Importer

To provide conformity of children Toys with Gulf Technical Regulations in force, the toys shall be tested and evaluated according to the related Gulf standards. In the event that there is no related standard, the tests determined by the Notified Body shall be performed following the approval of Gulf Conformity Assessment Committee. 

These examinations and tests shall be carried out, at the choice of the importer either by examination and testing of every toy or by examination and testing of the toys on a statistical basis.
Having regard to the risk analyze of the manufacturer, sample selection on statistical basis shall be made in order to supply homogeneity according to the guides of CR 14379 Classification of Children Toys and ISO-TR_8124-8_Safety of Children Toys. Tests are performed for first consignment, in case of any complaint and every 12 months.

If a consignment is accepted, all toys of the consignment shall be considered approved, except for those toys from the sample that have been found not to satisfy the tests.

If a consignment is rejected, appropriate measures are taken by TSE and the relevant authorities to prevent that the consignment is placed on the market. In the event of the frequent rejection of lots, the statistical verification is suspended and appropriate measures shall be taken.

In the event that Conformity Assessment results are positive, Conformity Declaration according to Regulation Clause 15(2) shall be issued by the importer and Certificate of Conformity issued by the notified body. It is under the responsibility of the Notified Body to attach the Number of the Notified Body to the each notified children toy. Besides, Importers shall ensure that, while a toy is under their responsibility, storage or transport conditions do not jeopardize its compliance with the requirements set out in Article 10 and Annex II.

The certificate is sent to company electronically for checking 10 working day is given to the applicant for the confirmation. Applicant have to inform the TSE about changes in the application form and and invoice. If the applicant do not respond  in 10 working days, draft certificate is ıssued as original certificate with the signature or related TSE manager then sent to applicant.

Moreover  a written contract is signed by authorized person for  confirmation of test reports and goods, accepting all responsibility in case of any failure in Gulf market and customs.

If applicant submitted proforma invoice and inspection is done according to proforma invoice, before issuing certificate, commercial invoice is requested from company and proforma invoice and commercial invoice contents are compared.

Conformity assessment results shall be notified to the authorized bodies and the other notified bodies if necessary, according to External Notifications and Announcements Procedure. 
4.1.2.3.1. Physical Control

It is the process relation between the invoice and certificate/report  established/ verified and the  control process for information(brand, marking, packaging etc.) in complying with Article 11 of BD131704-01. During consignmets checking before shipping; marking ,brand and packaging controls are done in oder to connect the relation between  the certificates/test reports with consignmets stated in the  invoice. Photos of consignmets are are taken, 15.01.02.FR.055 Consignment Based Inspection Report  is filled and send to related TSE department with 15.01.02.FR.029 Inspection Result Notice Form.

If physical control result is failed;

· Applicant is obligated to present all missing information and  documents in 15 working days, if not application is evaluated as failed.

· Goods that have failure will be absolutely checked physically again.

4.2. Changes may effect the certification:

4.2.1. Certification requirements

The GSO standards on issue are subject to a 2-year transition period ( adopted and endorsed from the current issued international/ national standards). 

If the manufacturer does not apply to NB during the transition period defined by GSO in order to re-evaluate the products and review of certification, the certification may be withdrawn according to Conformity Assessment Services Finalizing Procedure. 
In general, if the certificate will not be updated within 6 months starting from the standard expiry date, it will be automatically terminated in GSO platform.

The NB shall keep itsef informed and apprise its clients regarding any changes with in the scope of standardization and generally acknowledged state of the art. 

If these changes indicate that approved type may no longer in compliance with the provisions of the valid GSO Technical Regulations, NB will decide on these changes whether require further investigation or not upon application of the client.

If further investigation (inspection of samples, testing, document review, etc.) is required the NB shall inform the manufacturer accordingly and the originally certified product is re-evaluated.  

Besides, within 12 months prior to the expiry date of the certificate,  the product is subjected to a re-evaluation for renewal of certificate and the process regarded as “New application”. 

In general; certificates are suspended due to failure in renewing before the expiry date. If it will not be renewed within 6 months starting from the expiry date, it will be automatically terminated in GSO platform. 

Upon certificate renewal, the old (renewed) certificate will be changed to "Superseded" status once the new certificate is published.

4.2.2. Modification made by manufacturer

The manufacturer shall inform TSE of all changes in approved type(s) / design(s) and QMS that may influence the conformity with essential requirements of the Gulf Technical Regulations in force or the conditions for validity of the certificate, in particular in case of a change to the manufacturing process, the raw materials or components of electrical equipment or toys.

Moreover, manufacturer shall not put products subjected to conformity assessment into market, unless all the changes are approved by TSE.

The difference between the modified product and the originally certified product shall be re-evaluated and the process follows the same steps as a new application if there is a significant change.
4.3 After Examining Processes

4.3.1 Certificate Tracking
The validation, annulment, withdrawal and suspension procedures of the Certificate shall be conducted according to Conformity Assessment Services Finalizing Procedure.
It is required for the GC Certificates to be registered in GSO Certificate Tracking System as of 1 June 2016. 
At the time of issuing the certificate, the Notified Body shall register the economic operator (manufacturer or importer) and certificate information in the database system provided by GSO for this purpose, following the currently valid instructions provided by GSO. 

In order to create a new certificate, it shall be uploaded the necessary information  through the below link: https://www.gso.org.sa/gcts/coc/form?certType=g-mark-toys&version=2&orgCode=gso
The GSO system will generate certificates and GCTS markings for use on the products. 

Certificate holder shall have GC marking (G-Mark logo) or complete GCTS affixed to each approved product/packaging under its responsibility. GC marking (G-Mark logo) or complete GCTS for products can be put on the instruction manual accompanying the products on a voluntary basis.

The individual product markings shall be provided to the client by TSE and inform him about their correct placement and use, as stipulated in  the relevant Gulf technical regulations and GSO_GCTS Rules for the Use of the GSO Conformity Tracking Symbol (GCTS) (https://www.gso.org.sa/en/conformity/conformity-tracking-system/)

Example of individual product marking:
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Details and further updates are available in the user guide at: All content - GCTS User Guide - GSO e-Services Documentation (atlassian.net)

*Guideline on Update Existing old Certificate (Published) to e-Certificate - GCTS User Guide - GSO e-Services Documentation (atlassian.net): 

https://gcc-gso.atlassian.net/wiki/spaces/GUG/pages/2248081410/Update+Existing+old+Certificate+Published+to+eCertificate
*Renew Old Certificate to New e-Certificate - GCTS User Guide - GSO e-Services Documentation (atlassian.net)

https://gcc-gso.atlassian.net/wiki/spaces/GUG/pages/2250211407/Renew+Old+Certificate+to+New+eCertificate

*Create an e-Certificate for an Existing Product - GCTS User Guide - GSO e-Services Documentation (atlassian.net)

https://gcc-gso.atlassian.net/wiki/spaces/GUG/pages/2251423769/Create+an+e-Certificate+for+an+Existing+Product
The manufacturer is responsible to keep The Type Examination Document, Conformity Declaration and Technical File at least for 10 Years.

Any applicable registration fees levied by GSO shall be collected from the client by the Notified Body, who will pay such fees directly to GSO on behalf of the client. 

When GCTS registrations are going to be expired on GSO platform due to financial issues or any other aspects, TSE informs the client in written about GCTS expiry notification to avoid suspension of notification. 

The e-certificates will be checked by Directive responsible/Reviewer before the NB approval stage in GSO platform.

If TSE determine the G MARK or GCTS-QR code is misused or unfair commercial used ( e.g. marking based on terminated certificates or certificates are not approved  by GSO etc. ) by the manufacturer, TSE informs the GCC organization.

4.3.2 Billing
Fees in return of services shall be invoiced according to Conformity Assessment Services Finalizing Procedure.
4.3.3 Communication
Every kind of communication with authorized bodies and with other notified bodies shall be carried out according to External Notifications and Announcements Procedure. If necessary, free technical support to GSO shall be provided by TSE technical staff. Support for Legal issues shall be provided by GCC Legal Representative who is not responsible for any stages in certification process (application, evaluation etc.). If there is withdrawal of certificate due to product safety aspects, GSO will be informed by the Directive Responsible
5. RELATED DOCUMENTS AND REGISTRATIONS

Toys Safety Directive 2009/48/EEC (EN)

GCC Technical Regulation on Children Toys (BD131704-01)

TSE - Yönerge (002)  Belgelendirme Yönergesi (TSE - Guideline (002) Certification Guideline)

İlgili Değerlendirme Usul ve Esasları (related Procedures and Principles)

Conformity Assessment Application Procedure
Module B Conformity Assessment Procedure
DB-TSD-FR-009 Toy Safety Warnings languages comparison table

Conformity Assessment Services Finalizing Procedure
External Notifications and Announcements Procedure 

Sampling Method

Qualification and Assignment Method of Directives Experts

Toys Conformity Assessment Application Form 

Assessment Form of Technical File for Children Toy
GCC Technical Regulation on Children Toys (BD131704-01) Essential Requirements Conformity Assessment Report
Children Toys - External Document List

Children Toys – Expert List

DB List of Subcontractors (Laboratories) 

6. FLOW CHARTS
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ÜRETİCİ İÇİN BELGELENDİRME İŞLEMLERİ AKIŞ ŞEMASI

ÜRÜN STANDART 
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EVET
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TESTLERİ BELİRLER VE ONAYLANMIŞ 

KURULUŞUN ONAYIYLA TESTLER 

GERÇEKLEŞTİRİLİR.

EVET

HAYIR

ÜRETİCİ, TİP İLE ÜRETİMİN UYGUNLUĞUNU 

SAĞLAR VE 2009/48/EEC ANNEX III VE BD 

131704-01 ARTICLE 15(1)¶E GÖRE UYGUNLUK 

BEYANI HAZIRLAR.

ONAYLANMIŞ KURULUŞ TİP 

İNCELEME BELGESİ 

DÜZENLER.

HAYIR

TAMAMEN 

UYGUN

ÜRETİCİ TİP İNCELEME BELGESİ, 

UYGUNLUK BEYANI VE TEKNİK DOSYAYI 

10 YIL MUHAFAZA EDER.

TESTLERİN SONUÇLARI UYGUN 

MU?

EVET

HARİCİ BİLDİRİMLER 

PROSEDÜRÜNE GÖRE İŞLEM 

YÜRÜTÜLÜR.

HAYIR

(EN FAZLA

 10 İŞ GÜNÜ)
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İTHALATÇI İÇİN BELGELENDİRME İŞLEMLERİ AKIŞ ŞEMASI
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İTHALATÇI BD 131704-01 
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DOSYAYI 10 YIL MUHAFAZA EDER.

KOMİTE TARAFINDAN 

ONAYLANAN TESTLERİN 

SONUÇLARI UYGUN MU?

EVET

HARİCİ BİLDİRİMLER 
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YÜRÜTÜLÜR.

HAYIR


ACTION IS TAKEN IN ACCORDANCE WITH THE External Notifications and Announcements Procedure





PRODUCER





THE MANUFACTURER ENSURES THE CONFORMITY OF THE TYPE AND PRODUCTION AND SHALL ENSURE THAT THE TOY İS ACCOMPANİED BY İNSTRUCTİONS AND SAFETY INFORMATİON İN ARABİC LANGUAGE AND DRAFTS A DECLARATİON OF CONFORMITY IN ACCORDANCE WITH 2009/48/EEC ANNEX III AND BD 131704-01 ARTICLE 15(1)











(10 DAYS AT MOST)





CERTIFICATION FLOW CHART FOR THE PRODUCER





YES





YES





YES





NO





NO





NO





COMPLIES IN FULL








DO THE RESULTS OF THE TEST CONFORM?














THE MANUFACTURER MAINTAINS THE EYPE EXAMINATION DOCUMENT, CONFORMITY DECLARATION AND TECHNICAL FILE FOR 10 YEARS





TSE DETERMINES THE TESTS PROVIDING THE CONFORMITY OF THE REGULATION WITH THE TECHNICAL REQUIREMENTS AND SUBMIT TO THE APPROVAL of GULF CONFORMITY ASSESSMENT COMMITTEE








TSE UPLOAD THE TYPE EXAMINATION DOCUMENT and CREATES E-CERTIFICATES in the GSO PLATFORM 








IS THERE A PARTIAL OR FULL NONCONFORMITY?





IS THE PRODUCT IN SCOPE OF THE STANDARD?





CERTIFICATION FLOW CHART FOR THE IMPORTER








ACTION IS TAKEN IN ACCORDANCE WITH THE EXTERNAL NOTIFICATIONS AND ANNOUNCEMENTS PROCEDURE





NO





YES





TSE CREATES E- CERTIFICATE OF CONFORMITY AND ENSURES THE GULF CONFORMITY MARK ARE ATTACHED TO EACH TOY İN ACCORDANCE WİTH ARTICLE 16





THE IMPORTER SHALL ENSURE THAT THE TOY IS ACCOMPANİED BY İNSTRUCTİONS AND SAFETY İNFORMATİON İN ARABİC LANGUAGE AND ESTABLİSH THE TECHNİCAL DOCUMENTATİON PURSUANT TO ARTİCLE 20 AND DRAFTS A DECLARATION OF CONFORMITY IN ACCORDANCE WITH 2009/48/EEC ANNEX III AND BD 131704-01 ARTICLE 15(2)





THE IMPORTER MAINTAINS THE CERTIFICATE, CONFORMITY DECLARATION AND TECHNICAL FILE FOR 10 YEARS

















NO





COMPLIES IN FULL








IS THERE A PARTIAL OR FULL NONCONFORMITY?





TSE DETERMINES THE TESTS PROVIDING THE CONFORMITY OF THE REGULATION WITH THE TECHNICAL REQUIREMENTS AND SUBMIT TO THE APPROVAL of GULF CONFORMITY ASSESSMENT COMMITTEE








DO THE RESULTS OF THE TESTS    CONFORM?





NO





YES





YES





IS THE PRODUCT IN SCOPE OF THE STANDARD?
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ÜRETİCİ
ÜRETİCİ İÇİN BELGELENDİRME İŞLEMLERİ AKIŞ ŞEMASI
ÜRÜN STANDART KAPSAMINDA MI?
TAMAMEN VEYA KISMEN UYGUNSUZLUK VAR MI?
EVET
ÜRETİCİ, REGÜLASYONUN TEKNİK GEREKLERİNE UYGUNLUĞU SAĞLAYACAK TESTLERİ BELİRLER VE ONAYLANMIŞ KURULUŞUN ONAYIYLA TESTLER GERÇEKLEŞTİRİLİR.
EVET
HAYIR
ÜRETİCİ, TİP İLE ÜRETİMİN UYGUNLUĞUNU SAĞLAR VE 2009/48/EEC ANNEX III VE BD 131704-01 ARTICLE 15(1)’E GÖRE UYGUNLUK BEYANI HAZIRLAR.
ONAYLANMIŞ KURULUŞ TİP İNCELEME BELGESİ DÜZENLER.
HAYIR
TAMAMEN UYGUN
ÜRETİCİ TİP İNCELEME BELGESİ, UYGUNLUK BEYANI VE TEKNİK DOSYAYI 10 YIL MUHAFAZA EDER.
TESTLERİN SONUÇLARI UYGUN MU?
EVET
HARİCİ BİLDİRİMLER PROSEDÜRÜNE GÖRE İŞLEM YÜRÜTÜLÜR.
HAYIR
(EN FAZLA
 10 İŞ GÜNÜ)



IS THE IMPORTER LINKED TO A MANUFACTURER?
YES
IS IMPORTER ABLE TO PROVIDE THE NECESSARY EVIDENCE ABOUT THE MANUFACTURER RESPONSIBILITIES LISTED IN PARAGRAPH 2 OF ARTICLE (4) OF THIS REGULATION.
NO
YES
NO
IMPORTER SHALL CARRY OUT THE IMPORTER CONFORMITY ASSESSMENT PROCEDURE MENTIONED IN CLAUSE 4.1.2.3.
SHALL ENSURE THAT THE 
APPROPRIATE CONFORMITY ASSESSMENT PROCEDURE HAS BEEN CARRIED OUT BY THE MANUFACTURER
SHALL ENSURE THAT THE MANUFACTURER 
HAS DRAWN UP THE TECHNICAL DOCUMENTATION, THAT THE TOY BEARS THE GULF CONFORMITY MARK AND IS ACCOMPANIED BY THE REQUIRED DOCUMENTS, AND THE MANUFACTURER HAS COMPLIED WITH THE REQUIREMENTS SET OUT IN ARTICLE 4(7) AND (8).



İTHALATÇI
İTHALATÇI İÇİN BELGELENDİRME İŞLEMLERİ AKIŞ ŞEMASI
ÜRÜN STANDART KAPSAMINDA MI?
TAMAMEN VEYA KISMEN UYGUNSUZLUK VAR MI?
EVET
ONAYLANMIŞ KURULUŞ REGÜLASYONUN TEKNİK GEREKLERİNE UYGUNLUK SAĞLAYACAK TESTLERİ BELİRLER VE KÖRFEZ UYGUNLUK DEĞERLENDİRME KOMİTESİNİN ONAYINA SUNAR.
EVET
HAYIR
İTHALATÇI BD 131704-01 ARTICLE 15(2)’YE UYGUN OLARAK UYGUNLUK BEYANI HAZIRLAR.
ONAYLANMIŞ KURULUŞ, UYGUNLUK BELGESİNİ HAZIRLAR VE HER OYUNCAĞA ONAYLANMIŞ KURULUŞ NUMARASININ VE KÖRFEZ UYGUNLUK MARKASININ İLİŞTİRİLMESİNİ SAĞLAR.
HAYIR
TAMAMEN UYGUN
İTHALATÇI UYGUNLUK BELGESİ, UYGUNLUK BEYANI VE TEKNİK DOSYAYI 10 YIL MUHAFAZA EDER.
KOMİTE TARAFINDAN ONAYLANAN TESTLERİN SONUÇLARI UYGUN MU?
EVET
HARİCİ BİLDİRİMLER PROSEDÜRÜNE GÖRE İŞLEM YÜRÜTÜLÜR.
HAYIR



